{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Pre-fit form","Dimensions"],"not_rendered":{"charts":0,"images":26,"macros":1,"external_links":0,"defined_names":4,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Pre-fit form","index":0,"n_rows":260,"n_cols":17,"rows_kept":260,"cut":false,"hidden":false,"merged":[[172,12,172,15],[167,12,167,15],[166,12,166,15],[216,12,216,14],[110,10,110,11],[133,10,133,11],[161,12,161,15],[162,12,162,15],[171,12,171,15],[217,12,217,14],[1,1,1,16],[76,14,76,15],[77,14,77,15],[78,14,78,15],[79,14,79,15],[56,15,56,16],[51,2,52,13],[65,11,68,15],[69,11,73,15],[74,11,75,15],[83,14,83,15],[80,14,80,15],[81,14,81,15],[82,14,82,15],[109,10,109,11]]}
[]
[null,"Pre-fit form Lagooni Blue / Blue Extra"]
[]
[null,"Dealer"]
[null,"Consultant"]
[null,"Delivery address"]
[null,"Reference no."]
[null,"Phone no."]
[null,"Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Do you have any questions during the fitting? "]
[null,"Client",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Call us at + 31 (0) 174-281551"]
[]
[null,"Please fill in the fitting form as completely as possible. In case of missing data, the responsibility lies with the party who filled in the form. "]
[null,"SW: Seat width",null,null,"SH: Seat height"]
[null,"SD: Seat depth",null,null,"LLL:Lower leg length"]
[]
[null,"●","= These components are chosen if a basic configuration is to be made. "]
[]
[null,null,"Frame "]
[null,null,"Choose 1 type of frame, use the flowchart model selection tool if the choice of frame type is not clear."]
[null,null,"▫ Frame Lagooni Blue: push model with castors"]
[null,null,"▫ Frame Lagooni Blue Extra: push model with castors, extra wide frame"]
[null,null,"▫ If the SD < 43 cm, choose to remove the curved support tube."]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,"●","CFRA10",null,"Frame Lagooni Blue with backrest adjustment"]
[null,"●","CFRA11",null,"Frame Lagooni Blue Extra with backrest adjustment"]
[null,null,"AFRA10",null,"Remove curved support tube"]
[null,null,"AFRA11",null,"Other frame colour"]
[null,null,"AFRA14",null,"Lower frame * "]
[null,null,null,null,"Seat height: with 100 mm castors up to 60 cm, with legs up to 48 cm. If lower desired, choose a customised frame."]
[null,null,"CFRA04",null,"Custom frame *"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Wheels"]
[null,null,"▫ With 125 mm wheels, the seat height range is: 62 cm (with a standard seat cushion: 8 cm thick). The seat height is measured from the ground to the top of the seat."]
[null,null,"▫ Take the seat height into account if the shower/toilet wheelchair needs to be driven over a toilet bowl."]
[null,null,"CWIE4-100R",null,"100 mm castors with brake"]
[null,"●","CWIE4-125R",null,"125 mm castors with brake"]
[null,null,"-",null,"Without castors (on legs)"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Seat"]
[null,null,"▫ Width Lagooni Blue: 40 / 42 / 44 / 46 cm"]
[null,null,"▫ Width Lagooni Blue Extra: 48 / 50 / 52 / 54 cm"]
[null,null,"▫ Standard seat thickness Lagooni Blue: 8 cm  (minimaal 6 cm)."]
[null,null,"▫ Standard seat thickness Lagooni Blue Extra: 10 cm  (minimaal 8 cm)."]
[null,null,"▫  If you require a seat depth < 43 cm, please take into account the bar at the front that could potentially get in the way. If necessary, choose a padded backrest to achieve a seat depth of less than 43 cm."]
[]
[null,null,"▫ Properties neoprene: soft, stiffer than platilon, suitable in combination with decubitus wounds."]
[null,null,"▫ Properties platilon: strong, smoother than neoprene, suitable in combination with transfer board."]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,"●","CZIT01",null,"Seat upholstered with polyether and neopreen or platilon *"]
[]
[]
[null,null,"CZIT07",null,"Filler piece"]
[null,null,"CZIT08",null,"Abduction bobbin *"]
[null,null,"AZIT01E",null,"Extra seat adjustments *",null,null,null,null,null,null,null,null,"Inch","cm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1,2.54]
[]
[null,null,null,"Example"]
[null,null,null,"Opening front/back",null,null,"Opening front/back",null,"Opening front/back",null,null,"* Please note that a corner line runs at the back of the frame. Please take this into account if you opt for a opening at the back."]
[null,null,null,"Shape: taperd",null,null,"Shape: keyhole",null,"Shape: straight slot"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Please state the dimensions (cm) of the recess below. There is a surcharge for a recess on the left or right side. If the place/shape (for example wedge in the seat) differs from the examples above, please enclose a drawing including dimensions."]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Fields marked with * are REQUIRED. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,"* A:"]
[null,null,null,null,null,null,null,null,null,null,null,"* B:"]
[null,null,null,"Opening middle/deviating",null,null,"Opening left/right",null,"Opening front/back",null,null,"* C:"]
[null,null,null,"Shape: oval",null,null,"Shape: oval",null,"Shape: ellipse",null,null,"* D:"]
[null,null,null,null,null,null,null,null,null,null,null,"* E:",null,null,null,null,"(<7 cm not possible)"]
[null,null,null,null,null,null,null,null,null,null,null,"F:"]
[null,null,null,null,null,null,null,null,null,null,null,"* Location opening:"]
[null,null,null,null,null,null,null,null,null,null,null,"* Shape opening:"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Comments:"]
[]
[]
[]
[]
[]
[]
[null,null,"Backrestbracket"]
[null,null,"▫ The width of the backrest bracket is as wide as the width of the seat. "]
[null,null,"▫ The standard height of a backrest bracket is 48 cm."]
[null,"●","CRUG01",null,"Backrest bracket"]
[null,null,"CRUG01-M ",null,"Backrest bracket custom made *"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Backrest"]
[null,null,"▫ The standard height of a backrest canvas is 30 cm."]
[null,null,"▫ If an upholstered backrest is chosen, the following applies: seat depth + 3 cm."]
[null,null,"▫ For a 'standard' upholstered backrest the following applies: width of the upholstered back = backrest bracket + 2 cm."]
[null,null,"▫ Properties neoprene: soft, stiffer than platilon, suitable in combination with decubitus wounds."]
[null,null,"▫ Properties platilon: strong, smoother than neoprene, suitable in combination with transfer board."]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,"●","CRUG12",null,"Backrest canvas, black"]
[null,null,"CRUG01B",null,"Backrest upholstered with polyether and neoprene or platilon *"]
[]
[]
[null,null,"CRUG01BZIJ",null,"Backrest upholstered with side support with polyether and neoprene or platilon * "]
[]
[]
[null,null,"CRUG01K",null,"Backrest upholstered contour with polyether and neoprene or platilon * "]
[]
[]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Armrest"]
[null,null,"▫ The armrests are swing-away and removable."]
[null,null,"▫ The height of the armrest is measured from top edge of seat to top edge of armrest."]
[null,null,"▫ For shorter and lower armrests, you can choose a junior armrest (see size sheet tab) or a custom-made armrest."]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,null,"CARM03-15",null,"Junior armrest straight H15 cm"]
[null,null,"CARM03-18",null,"Junior armrest straight H18 cm"]
[null,null,"CARM01",null,"Armrest single bend H23 cm"]
[null,"●","CARM02",null,"Armrest extra strong H23 cm "]
[null,null,"CARM04",null,"Armrest custom-made *"]
[null,null,"CARM09",null,"Armrest with extra horizontal bend"]
[null,null,"AARM02E",null,"Additional work armrests (lower) *"]
[null,null,"-",null,"No armrests"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Armpad"]
[null,null,"▫ Properties neoprene: soft, stiffer than platilon, suitable in combination with decubitus wounds."]
[null,null,"▫ Properties platilon: strong, smoother than neoprene, suitable in combination with transfer board."]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,"●","CARM05",null,"Armpads PU"]
[null,null,"CARM06",null,"Armpads upholstered"]
[]
[]
[null,null,"AARM06E",null,"Extra labour upholstered armpads *"]
[null,null,"-",null,"No armpads"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Legrest and footplate"]
[null,null,"▫ Properties neoprene: soft, stiffer than platilon, suitable in combination with decubitus wounds."]
[null,null,"▫ Properties platilon: strong, smoother than neoprene, suitable in combination with transfer board."]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,"●","CBE01SET",null,"Swing-away legrest with flip-up footplate",null,null,null,null,null,null,null,"Toilet bowl height - A (cm):"]
[null,null,"CBE02SET",null,"Elevating legrest with flip-up footplate"]
[null,null,"CBE04SET",null,"Elevating legrest, upper part (for amputation)"]
[null,null,"CVOE03",null,"One-piece footrest, upholstered (mounting footrest with clamps)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Bottom of seat - B (cm):"]
[null,null,"CVOE04B",null,"Upholstery one-piece footplate Lagooni Blue"]
[null,null,null,null,"- In combination with swing-away legrest"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Lower leg length - C (cm):"]
[]
[null,null,"LVOE06",null,"Upholstery one-piece footplate Lagooni Blue Extra (extra wide)"]
[null,null,null,null,"- In combination with swing-away legrest"]
[]
[]
[]
[]
[null,null,"CVOE09",null,"Upholstery two-piece footplate Lagooni Blue "]
[]
[]
[null,null,"CVOE12",null,"Upholstery two-piece footplate Lagooni Blue Extra (extra breed)"]
[]
[]
[null,null,"AVOE01E",null,"Extra adjustments upholstered footplate * "]
[null,null,"-",null,"No legrest or footplates"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Headrest "]
[null,null,"▫ If a headrest is needed, it is recommended to choose a upholstered backrest. "]
[null,null,"▫ Properties neoprene: soft, stiffer than platilon, suitable in combination with decubitus wounds."]
[null,null,"▫ Properties platilon: strong, smoother than neoprene, suitable in combination with transfer board."]
[null,null,"CSTE02",null,"Headrest upholstered "]
[]
[]
[null,null,"CSTE03K",null,"Headrest PU Small"]
[null,null,"CSTE03MG",null,"Headrest PU Medium"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Lateral support"]
[null,null,"▫ Length of pelvic belt: from rotary knob back angle adjustment left to rotary knob back angle adjustment right."]
[null,null,"▫ Properties neoprene: soft, stiffer than platilon, suitable in combination with decubitus wounds."]
[null,null,"▫ Properties platilon: strong, smoother than neoprene, suitable in combination with transfer board."]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,null,"CSTE01L",null,"Lateral support upholstered with mounting kit, left * "]
[]
[]
[null,null,"CSTE01R",null,"Lateral support upholstered with mounting kit, right *"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Length pelvic belt (cm):"]
[null,null,"CGOR02",null,"Pelvic belt"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Leg protection"]
[null,null,"▫ Properties neoprene: soft, stiffer than platilon, suitable in combination with decubitus wounds."]
[null,null,"▫ Properties platilon: strong, smoother than neoprene, suitable in combination with transfer board."]
[null,null,"CKUI01",null,"Adjustable calf strap neopreen"]
[null,null,"CKUI02",null,"Calf protector for frame tube, upholstered"]
[]
[]
[null,null,"CKUI03",null,"Adjustable calf strap bisonyl"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Insertion rails stainless steel"]
[null,null,"▫ The rails protrude 3 cm below the seat. Take this into account when determining the seat height."]
[null,null,"CTOO03",null,"Insertion rails for bedpan / toiletbucket Ø 30 cm"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Bedpan / toilet bucket "]
[null,null,"▫ When rinsing the intestines, it is advised to choose a toilet bucket because of the size of the bucket."]
[null,null,"CTOO02",null,"Bedpan with lid, stainless steel"]
[null,null,"CTOO04",null,"Toilet bucket with lid, stainless steel"]
[]
[null,"Comments:"]
[]
[]
[]
[null,null,"Accessories"]
[null,null,"* Please enter the required measurements in the \"Dimensions\" tab."]
[null,null,"CTOO01SP",null,"Splash skirt (bisonyl) *"]
[null,null,"CTAF01",null,"Tabletop transparent with accessories *"]
[null,null,"CBED01",null,"Bedhook and receiver"]
[]
[null,"Comments:"]

{"sheet":"Dimensions","index":1,"n_rows":191,"n_cols":21,"rows_kept":191,"cut":false,"hidden":false,"merged":[[177,4,177,6],[181,2,182,23],[188,4,188,6],[189,4,189,6],[190,4,190,6],[176,4,176,6],[148,15,148,16],[148,17,148,19],[149,15,149,16],[149,17,149,19],[150,15,150,16],[150,17,150,19],[151,15,151,16],[151,17,151,19],[152,15,152,16],[152,17,152,19],[145,15,145,16],[145,17,145,19],[146,15,146,16],[146,17,146,19],[147,15,147,16],[147,17,147,19],[143,15,144,19],[64,18,65,21],[64,22,65,23],[75,18,77,23],[78,18,79,21],[78,22,79,23],[80,18,81,21],[80,22,81,23],[82,18,83,21],[82,22,83,23],[92,6,92,17],[93,6,97,17],[123,16,127,21],[62,18,63,21],[62,22,63,23],[30,10,30,13],[31,10,31,13],[32,10,32,13],[33,10,33,13],[34,10,34,13],[35,10,35,13],[36,10,36,13],[57,18,59,23],[60,18,61,21],[60,22,61,23],[29,10,29,13],[4,9,4,13],[5,10,5,13],[10,9,12,23],[13,9,16,23],[23,9,24,13],[25,10,25,13],[26,10,26,13],[27,10,27,13],[28,10,28,13]]}
[]
[null,null,"Backrest"]
[]
[null,null,"Upholstered backrest"]
[null,null,null,null,null,null,null,null,null,"Upholstered backrest"]
[null,null,null,null,null,null,null,null,null,"C:"]
[null,null,null,null,null,null,null,null,null,"(Minimum 15 cm, maximum 40 cm)"]
[]
[]
[null,null,null,null,null,null,null,null,null,"Note:"]
[null,null,null,null,null,null,null,null,null,"- With a padded backrest, the effective seat depth is reduced by 3 cm."]
[]
[]
[null,null,null,null,null,null,null,null,null,"- A padded backrest is 2 cm wider than the backrest bracket and therefore also the seat width. Take this into account when completing the tables below."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Upholstered backrest with lateral support",null,null,null,null,null,null,"Upholstered backrest with lateral support"]
[]
[null,null,null,null,null,null,null,null,null,"Dright :"]
[null,null,null,null,null,null,null,null,null,"Eleft : "]
[null,null,null,null,null,null,null,null,null,"F:"]
[null,null,null,null,null,null,null,null,null,"Gright :"]
[null,null,null,null,null,null,null,null,null,"Gleft :"]
[null,null,null,null,null,null,null,null,null,"Hright :"]
[null,null,null,null,null,null,null,null,null,"Hleft :"]
[null,null,null,null,null,null,null,null,null,"Iright :"]
[null,null,null,null,null,null,null,null,null,"Ileft :"]
[null,null,null,null,null,null,null,null,null,"Jright :"]
[null,null,null,null,null,null,null,null,null,"Jleft :"]
[null,null,null,null,null,null,null,null,null,"K:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"ARMREST"]
[null,null,"Type armrest"]
[null,null,"Armrest type: extra strong, single bend & horizontal bend"]
[]
[null,null,"Extra strong",null,null,null,"Single bend"]
[null,null,"Height AH: customised ",null,null,null,"Height AH: customised "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AH - Height custom armrest (cm)"]
[null,null,null,null,null,null,null,null,null,null,null,"Horizontal bend"]
[null,null,null,null,null,null,null,null,null,null,null,"Example left armrest with horizontal bend in front."]
[null,null,null,null,null,null,null,null,null,null,null,"Height AH: customised ",null,null,null,null,null,null,"Extra strong:"]
[null,null,null,null,null,null,null,null,null,null,null,"Length AL: customised"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Single bend:"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Horizontal bend:"]
[]
[]
[]
[]
[]
[null,null,"Extra strong",null,null,null,"Single bend"]
[null,null,"Length AL: customised",null,null,null,"Length AL: customised"]
[null,null,"Standard AL extra strong: 32 cm",null,null,null,"Standard AL single bend: 32 cm"]
[null,null,null,null,null,null,"Standard AL Junior: 24 cm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AL - Length custom armrest (cm)"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Extra strong:"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Single bend:"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Horizontal bend:"]
[]
[]
[]
[null,null,"Type armpad"]
[null,null,"Armpad type: PU & upholstered."]
[]
[]
[null,null,"PU armpad"]
[]
[null,null,null,null,null,null,"Note:"]
[null,null,null,null,null,null,"The PU armrests are available in a standard size of 25 cm. If a different size is required, choose a padded armrest. The armrests are adaptable for the extra strong armrests as well as the armrests with single bend and the armrests with horizontal bend. Enter the required dimensions in the table at the end of this document. "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Length: 25 cm (standard)"]
[]
[]
[]
[null,null,"Upholstered armpad"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Length: 25 cm",null,null,null,"Length: 30 cm",null,null,null,null,"Length: 35 cm",null,null,null,null,"Length: customized"]
[null,null,null,null,null,null,"5cm extended backwards",null,null,null,null,"10 cm extended backwards"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Junior armrests are lower and shorter than the extra strong armrests & armrests with single bend. Please take this into account when choosing the armrest length."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Junior model",null,null,null,"Junior model",null,null,null,null,"Junior model "]
[null,null,"Length: 20 cm",null,null,null,"Length: 25 cm",null,null,null,null,"Length: 30 cm"]
[null,null,null,null,null,null,"5 cm extended backwards",null,null,null,null,"10 cm extended backwards"]
[]
[]
[]
[]
[null,null,"Upholstered armrest width (C1) is 6 cm wide as standard.",null,null,null,null,null,null,null,null,"Upholstered armrest width (C1) is 6 cm wide as standard."]
[null,null,"Example: Front armrest bend: left (Junior model)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Measurements armrest & armpad (cm)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A:",null,{"$f":"IF(W61,W61,IF(W63,W63,IF(W65,W65,\"Standard 23\")))","v":"Standard 23"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C1:",null,null,null,null,"(C1 & C2: minimum 6 cm, maximum 12 cm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C2:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D1",null,null,null,null,"(D1: minimum 4 cm, maximum 10 cm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D2",null,null,null,null,"(D2 = E + minimum 4 cm)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Extend to:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Armrest horizontal bend",null,null,null,"Armrest horizontal bend",null,null,null,null,"Measurements hemiplegic armrest"]
[null,null,"Height (AH):",null,"15/18/23/... cm",null,"Height (AH):",null,"15/18/23/... cm"]
[null,null,"Length armpad (B):",null,"20 cm",null,"Length armpad (B):",null,null,"25 cm"]
[null,null,"Width armpad (C1):",null,"6 cm",null,"Width armpad (C1):",null,null,"6 cm"]
[]
[]
[]
[null,null,"ACCESSORIES"]
[null,null,"Splash skirt"]
[null,null,"A Splash skirt is made of bisonyl. It is mounted under the seat. Fill in the width and height of the splash skirt below."]
[]
[null,null,"Measurements in cm"]
[null,null,"Height"]
[null,null,"Width"]
[]
[]
[null,null,"Table top"]
[null,null,"A table top is fitted under the armrest using a receiving tube and fastened with a star knob. Indicate below which side the table top should fold away. Then also indicate the dimensions of the table top and the stomach recess."]
[]
[]
[]
[]
[]
[null,null,"Measurements in cm"]
[null,null,"Total width",null,null,null,null,null,null,"The minimum total width of the table top is seat width + 10 cm."]
[null,null,"Total depth",null,null,null,null,null,null,"The maximum depth of the table top is 60 cm."]
[null,null,"Belly recess",null,null,null,null,null,null,"Belly recess: measure from the back of the tabletop to the front of the Belly."]